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Product overview
The AXQ-100C belongs to an automatic mounting series intended for batch specimen preparation. An isolated mounting chamber is managed through programmed control of process conditions, including temperature and time. The machine supports hot mounting with thermosetting and thermoplastic materials. Mounting configurations in 25, 30 and 40 mm diameters can be selected according to the specimen and preparation requirements.
Specifications
	Model
	AXQ-100C

	Machine body
	Benchtop

	Mounting chamber
	Two isolated preparation chambers

	Mounting method
	automatic 

	Pressure loading and release
	automatic  (pneumatic )

	Temperature control
	automatic 

	Specimen lift
	automatic  (pneumatic )

	Specimen size
	Φ25mm/Φ30mm/Φ40mm

	Control system
	touchscreen

	End of preparation
	Automatic stop

	Cooling method
	Natural cooling

	Heater specification
	8000W*2

	Temperature range
	0-300℃

	Pressure range
	0-2MPA (specimen preparation pressure 0-72MPA)

	Heating time
	0-99 min (adjustable)

	Air pressure
	0.5-0.8 MPa

	Control power supply
	220V

	Dimensions
	460*410*500mm (L * W * H)

	Net weight
	35KG

	Gross weight
	45KG

	Standard configuration
	

	Main unit
	1 unit

	Mounting mold
	2 sets (inside main unit)

	Mounting material
	1 container (500mL)

	Technical documents
	1 set (manual, warranty card and inspection certificate)

	Options
	Air pump


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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