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Product overview
The AXQ-2Q embeds small metallographic specimens in thermosetting plastic under heat and pressure. It is intended for samples whose size or irregular shape makes direct handling difficult. Forming a mount around the specimen makes subsequent grinding and polishing easier and provides a convenient specimen form for examining the microstructure with a metallographic microscope.
Specifications
	Model
	AXQ-2Q

	Machine body
	Benchtop

	Mounting chamber
	Single preparation chamber

	Mounting method
	automatic 

	Pressure loading and release
	automatic  (pneumatic )

	Temperature control
	automatic 

	Specimen lift
	automatic  (pneumatic )

	Specimen size
	Φ25mm/Φ30mm/Φ40mm (choose one)

	Control system
	Digital temperature and time controller

	End of preparation
	Audible buzzer

	Cooling method
	

	Heater specification
	800W

	Temperature range
	Room temperature-210℃

	Pressure range
	

	Heating time
	

	Air pressure
	0.5-0.7 MPa

	Control power supply
	220V

	Dimensions
	350*300*400mm (L * W * H)

	Net weight
	15KG

	Gross weight
	25KG

	Standard configuration
	

	Main unit
	1 unit

	Mounting mold
	1 set (inside main unit)

	Mounting material
	1 container (500mL)

	Technical documents
	1 set (manual, warranty card and inspection certificate)

	Options
	Air pump


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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