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Product overview
The AXQ-50Y uses an integrated floor-standing structure for metallographic specimen mounting. It supports thermosetting and thermoplastic mounting media, with programmed management of the heating, timing and cooling stages. Mounting sizes listed for the machine are 25, 30, 40 and 45 mm in diameter. A version with interchangeable steel mould sleeves is available as an option for changing the mounting size.
Specifications
	Model
	AXQ-50Y

	Machine body configuration
	Integrated floor-standing unit

	Mounting chamber
	Single preparation chamber

	Control system
	Color touchscreen, PLC control

	Mounting method
	automatic 

	Pressure loading and release
	automatic  (hydraulic )

	Temperature control
	automatic 

	Specimen lift
	automatic 

	Cooling method
	Recirculating water cooling with automatic timing

	Mounting size
	Φ25mm/30mm/40mm/45mm/50mm (other sizes available to order)

	Heating power
	1750W

	Temperature range
	Room temperature - 210℃

	Pressure time
	0 - 99min (adjustable)

	Tank capacity
	40L

	Power supply
	220V

	Dimensions
	700*560*1250mm (L * W * H)

	Net weight
	90KG

	Gross weight
	100KG

	Standard configuration
	

	Main unit
	1 unit

	Cooling system
	1 set

	Mounting mold
	1 set (inside main unit)

	Feed funnel
	1 units

	Mounting material
	1 container (500ml)

	Power cable
	1 piece

	Technical documents
	1 set (manual, warranty card and inspection certificate)


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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