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Product overview
The AXQ-5S is designed for metallographic specimen preparation by hot mounting. Its control system combines a touchscreen interface with a PLC to manage the mounting process, including temperature, time and cooling. Thermosetting and thermoplastic filling materials are supported. The machine brings these process controls together for preparing mounted specimens according to the selected material and mounting requirements.
Specifications
	Model
	AXQ-5S

	Machine body
	Benchtop

	Mounting chamber
	Single mounting chamber

	Control system
	Color touchscreen, PLC control

	Mounting method
	automatic 

	Pressure application
	automatic  (hydraulic )

	Temperature control
	automatic 

	Specimen lift
	automatic 

	Cooling method
	automatic water cooled

	End of preparation
	Automatic shutdown

	Specimen size
	Φ25mm/30mm/40mm/45mm (not interchangeable)

	Heating power
	1300W

	Temperature range
	Room temperature - 210℃

	Heating time
	0 - 99min (adjustable)

	Control power supply
	220V

	Dimensions
	360*400*550mm (L * W * H)

	Net weight
	28.5KG

	Gross weight
	40KG

	Standard configuration
	

	Main unit
	1 unit

	Mounting mold
	1 set (inside main unit)

	Feed funnel
	1 piece

	Mounting material
	1 container (500ml)

	Power cable
	1 piece

	Instruction manual
	1 copy

	Warranty card
	1 copy

	Inspection certificate
	1 copy

	Notes
	Optional water tank


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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