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Product overview
The AXQ-5Y is designed as an integrated floor-standing machine for batch metallographic mounting. A colour touchscreen and PLC control manage temperature, time and cooling during the mounting process. The machine supports both thermosetting and thermoplastic mounting media. Hot-mounting moulds can be changed to suit the specimen, and the machine can mount two specimen blocks simultaneously.
Specifications
	Model
	AXQ-5Y

	Machine body
	Benchtop

	Mounting chamber
	Single mounting chamber

	Control system
	Color touchscreen, PLC control

	Mounting method
	automatic 

	Pressure application
	automatic  (hydraulic )

	Temperature control
	automatic 

	Specimen lift
	automatic 

	Cooling method
	automatic water cooled

	End of preparation
	Automatic shutdown

	Specimen size
	Φ25mm/30mm/40mm/45mm (other sizes available to order; interchangeable)

	Heating power
	1600W

	Temperature range
	Room temperature - 210℃

	Heating time
	0 - 99min (adjustable)

	Control power supply
	220V

	Dimensions
	550*560*450mm (L * W * H)

	Net weight
	65KG

	Gross weight
	80KG

	Standard configuration
	

	Main unit
	1 unit

	Mounting mold
	1 set (inside main unit)

	Feed funnel
	1 piece

	Mounting material
	1 container (500ml)

	Power cable
	1 piece

	Instruction manual
	1 copy

	Warranty card
	1 copy

	Inspection certificate
	1 copy

	Notes
	Optional water tank


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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