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Product overview
Specimens are placed in UV-transparent mounting moulds and surrounded with a suitable UV-curing resin. The GX-40 uses an LED-based illumination system to cure the resin and form a transparent mount. A cooling arrangement is incorporated for the curing and cooling process. This provides a light-curing route for preparing mounted metallographic specimens for subsequent handling and examination.
Specifications
	Model
	GX-40

	Machine body
	Benchtop

	Mounting method
	Light curing

	Control system
	Color touchscreen, PLC control

	Power
	Low / medium / high

	Time
	Adjustable

	Cooling method
	automatic 

	End of preparation
	Automatic ejection

	Maximum specimens
	24 molds of Φ30mm; 15 molds of Φ40mm

	Maximum specimen height
	40mm

	LED wavelength
	365nm

	Curing time
	60 s (example using M789001 light-curing agent)

	Curing temperature
	70-90 °C (example using M789001 light-curing agent)

	Control power supply
	AC100-240 V ，50/60 Hz

	Machine dimensions
	420*410*200mm (L * W * H)

	Machine weight
	16KG

	Standard configuration
	

	Main unit
	1 unit

	UV light source
	1 set

	Mounting mold
	White flexible silicone molds: 3 each of Φ30 mm and Φ40 mm

	Mounting material
	UV curing resin, 250 ml

	Tools
	1 each: stainless steel tweezers, measuring cup and funnel

	Power cable
	1 piece

	Technical documents
	1 set (manual, warranty card and inspection certificate)


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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