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Product overview
The MPD-1A has sealed water inlet and outlet arrangements that separate flowing water from the circuit board. A large, deep preparation chamber helps contain coolant and polishing-fluid splashes and accommodates larger specimens. Its constant-torque spindle offers continuously variable speed from 50 to 1500 rpm. Coarse grinding, fine grinding and polishing are supported through changes of abrasive paper and polishing disc for metals, ceramics, rocks and electronic components.
Specifications
	Model
	MPD-1A

	Machine body configuration
	Benchtop, single disc

	Control method
	Single disc, single control

	Rotation direction
	Forward and reverse rotation

	Grinding disc speed
	Stepless speed control (50-1500r/min) + preset speeds (400, 700, 900, 1400r/min)

	Main unit power
	750W

	Speed control
	Servo control

	Grinding disc diameter
	φ230mm (optional φ200)

	Water spray
	Adjustable orientation

	Power supply
	220V

	Dimensions
	360*560*270mm (L * W * H)

	Weight
	19.8KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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