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Product overview
The MPD-2A supports coarse grinding, fine grinding and polishing of metals, ceramics, rocks and electronic components. Its sealed water inlet and outlet arrangements separate the water path from the circuit board. The large, deep chamber helps contain coolant and polishing-fluid splashes while allowing easier handling of larger specimens. Abrasive papers can be changed readily, and different polishing discs can be selected for the preparation task.
Specifications
	Model
	MPD-2A

	Machine body configuration
	Benchtop, two discs

	Control method
	Two discs with independent controls

	Rotation direction
	Forward and reverse rotation

	Grinding disc speed
	Stepless speed control (50-1500r/min) + preset speeds (400, 700, 900, 1400r/min)

	Main unit power
	750W*2

	Speed control
	Servo control

	Grinding disc diameter
	φ230mm (optional φ200)

	Water spray
	Adjustable orientation

	Power supply
	220V

	Dimensions
	650*560*270mm (L * W * H)

	Weight
	30KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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