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Product overview
The Q-3 uses a manually operated lever for specimen cutting. It is intended for routine sampling of small and medium workpieces in metallographic and petrographic preparation, particularly in small and medium laboratories. The cutting arrangement is supported by a recirculating cooling system intended to manage cutting heat and help reduce burning of the cut surface during specimen preparation.
Specifications
	Model
	Q-3

	Maximum cutting diameter
	Φ50mm

	Cut-off wheel dimensions
	Φ250*1.5*Φ32mm

	Cutting modes
	manual 

	Cooling system
	automatic  (water cooled)

	Tank capacity
	65L

	Spindle speed
	3500r/min

	Motor power
	2.2KW

	Machine configuration
	Benchtop

	Power supply
	380V

	Weight
	150KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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