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Product overview
Built as an integrated floor-standing machine, the QG-100X supports precision sectioning of metals, ceramics, rocks and electronic components. Automatic coolant circulation accompanies the cutting process. The split, two-level positioning platform is designed for accurate placement of individual cuts and successive cuts, allowing specimen blocks or slices to be taken from a range of workpiece shapes for further preparation and examination.
Specifications
	Model
	QG-100X

	Control system
	Push buttons

	Door opening
	Front-opening lid

	Spindle speed
	2840r/min

	X table movement
	manual 50mm

	Clamping table
	Split table

	Y travel
	manual  (250mm)

	Maximum cutting dimensions
	130*380*100mm

	Cutting modes
	manual 

	Effective travel
	Up to 220mm (adjustable)

	Cutting table dimensions
	250*300mm

	Cutting speed
	manual 

	Feed method
	manual 

	Reset method
	manual 

	Feed rate
	manual 

	Cutting progress display
	/

	Maximum wheel dimensions
	φ350*2.5*φ32mm

	Cooling system
	Automatic water cooling, 4 channels

	Tank capacity
	60L

	Motor power
	4.0KW

	Machine configuration
	Integrated floor-standing unit

	Power supply
	380V

	Dimensions
	850*950*1350mm (L * W * H)

	Net weight
	300KG

	Gross weight
	350KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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