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Product overview
The QG-4A is intended for preparing conventional metallographic and petrographic specimens. Its automatic cooling tank supplies cooling during manual cutting. The design applies ergonomic principles to the operating arrangement, with an emphasis on convenient handling and low-noise operation. It provides a manual sectioning approach for laboratories preparing metal and rock specimens, with cooling incorporated into the specimen-cutting process.
Specifications
	Model
	QG-4A

	Maximum cutting diameter
	Φ85mm

	Cut-off wheel dimensions
	Φ300*2.0*Φ32mm

	Cutting modes
	manual 

	Cooling system
	automatic  (water cooled)

	Tank capacity
	40L

	Spindle speed
	2800r/min

	Motor power
	4KW

	Machine configuration
	Integrated floor-standing unit

	Power supply
	380V

	Weight
	250KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
image2.jpg




image1.jpg
CCCCCCCCCCCCCCCCCCC








