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Product overview
The QG-4T uses a manual lever-operated cutting arrangement for specimen preparation. Its floor-standing configuration includes a recirculating cooling system intended to manage cutting heat and help reduce burning of the cut surface. The machine is aimed at small and medium laboratories preparing conventional metallographic and petrographic samples, with a straightforward operating approach for routine sectioning work.
Specifications
	Model
	QG-4T

	Maximum cutting diameter
	Φ65mm

	Cut-off wheel dimensions
	Φ250*2.0*Φ32mm

	Cutting modes
	manual 

	Cooling system
	automatic  (water cooled)

	Tank capacity
	40L

	Spindle speed
	2800r/min

	Motor power
	2.2KW

	Machine configuration
	Integrated floor-standing unit

	Power supply
	380V

	Weight
	100KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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