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Product overview
The QG-5A combines manual cutting with automatic coolant circulation. Its split, two-level movable positioning platform supports both individual positioned cuts and successive positioned cuts. This arrangement is intended for taking specimen blocks and slices from different workpieces. Suitable specimen materials include metals, ceramics, rocks and electronic components, covering precision sampling tasks where the cut must be placed to suit the specimen.
Specifications
	Model
	QG-5A

	Control system
	Push buttons

	Door opening
	Front-opening lid

	Spindle speed
	2840r/min

	X table movement
	/

	Clamping table
	Fixed table

	Y travel
	manual  (250mm)

	Maximum cutting dimensions
	130*380*100mm

	Cutting modes
	manual 

	Effective travel
	Up to 220mm (adjustable)

	Cutting table dimensions
	200*300mm

	Cutting speed
	manual 

	Feed method
	manual 

	Reset method
	manual 

	Feed rate
	manual 

	Cutting progress display
	/

	Maximum wheel dimensions
	φ350*2.5*φ32mm

	Cooling system
	Automatic water cooling, 4 channels

	Tank capacity
	60L

	Motor power
	4.0KW

	Machine configuration
	Integrated floor-standing unit

	Power supply
	380V

	Dimensions
	850*950*1350mm (L * W * H)

	Net weight
	300KG

	Gross weight
	350KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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