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Product overview
An external handwheel drives bevel gears and a lead screw to move the lower mould within the steel sleeve. The specimen and thermosetting plastic are formed under heat, while an internal spring compensates the mounting pressure and an indicator lamp shows the pressure condition. The machine includes a digital temperature controller, thermocouple, time setting and buzzer. Mounted specimens can then be ground, polished and examined microscopically.
Specifications
	Model
	XQ-2B

	Machine body
	Benchtop

	Mounting chamber
	Single mounting chamber

	Mounting method
	manual 

	Pressure loading and release
	manual 

	Temperature control
	automatic 

	Specimen lift
	manual 

	Cooling method
	Natural cooling

	End of preparation
	Audible buzzer

	Mounting size
	Choice of Φ25mm, Φ30mm or Φ40mm

	Heater specification
	Φ25/Φ30mm：650W；Φ40mm：800W

	Temperature adjustment range
	Room temperature -300℃

	Timer
	0-99 min

	Power supply
	220V

	Dimensions
	320 * 280 * 420mm (L * W * H)

	Net weight
	22KG

	Gross weight
	32kg

	Standard configuration
	

	Main unit
	1 unit

	Mounting mold
	1 set

	Mounting material
	1 container (500mL)

	Power cable
	1 piece

	Technical documents
	1 set (manual, warranty card and inspection certificate)


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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