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Product overview
Using a touchscreen PLC system, the ZMP-1000D automatically controls the amount of material removed during grinding. It is intended for research work requiring controlled reduction in the thickness of precision components or preparation to a specified grinding depth. Its focus is on managing material removal as part of the specimen-preparation process.
Specifications
	Model
	ZMP-1000D

	Machine body configuration
	Benchtop (touchscreen PLC control)

	Clamping capacity
	4 specimens (custom specimen sizes available)

	Pressure application
	Pneumatic (individual / central loading)

	Operation
	Automatic / semi-automatic

	Control system
	Color touchscreen, PLC control

	Grinding method
	Programmed automatic / semi-automatic (two grinding modes)

	Grinding tracking
	Digital display and real-time plot

	Resolution
	1μm

	Grinding accuracy
	10μm/ (optional  2μm)

	Grinding disc speed
	50-1500 rpm

	Grinding head speed
	20-200 rpm

	Abrasive dosing
	Two-channel automatic dosing

	Dosing interval
	Programmable; minimum dosing interval 0.1S

	Dosing time
	Programmable; minimum spray interval 0.1S

	Preparation time
	0-9999 s

	Main unit power
	1200W

	Specimen preparation diameter
	Φ30mm (special sizes optional)

	Grinding disc diameter
	230mm

	Power supply
	220V/50HZ

	Dimensions
	650mm*500mm*680mm (L * W * H )

	Net weight
	71.5KG

	Gross weight
	82KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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