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Product overview
This floor-standing cutter uses a large colour touchscreen and PLC control. Its split, two-level movable platform supports positioned cutting and the preparation of thin flat sections from irregular workpieces. Feed travel can be set for the task, while cutting speed is continuously adjustable from 1 to 100 mm/min. Speed can also be adjusted during cutting in response to the cutting conditions.
Specifications
	Model
	ZQ-100X

	Control system
	8-inch color touchscreen, PLC control system

	Door opening
	Front-opening lid

	Spindle speed
	2840r/min

	X table movement
	manual 50mm

	Clamping table
	Split table

	Y travel
	automatic  / manual  (250mm)

	Maximum cutting dimensions
	130*380*100mm

	Cutting modes
	automatic  / manual 

	Effective travel
	Up to 220mm (adjustable)

	Cutting table dimensions
	250*300mm

	Cutting speed
	1 - 100mm / min (stepless speed control)

	Feed method
	Adjustable reciprocating cutting

	Reset method
	automatic  / manual 

	Feed rate
	0 - 200mm / minstepless speed control

	Cutting progress display
	LCD digital display (real-time)

	Maximum wheel dimensions
	φ350*2.5*φ32mm

	Cooling system
	Automatic water cooling, 4 channels

	Tank capacity
	60L

	Motor power
	4.0KW

	Machine configuration
	Integrated floor-standing unit

	Power supply
	380V

	Dimensions
	850*950*1350mm (L * W * H)

	Net weight
	300KG

	Gross weight
	350KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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