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Product overview
The ZXG-300 is designed for sampling special ceramics, crystals, electronic ceramic components, gemstones, rocks and glass. The touchscreen PLC system controls the cutting sequence for different specimen forms. Supported tasks include cutting square specimen bars and automatically producing successive thin slices. Both bar preparation and repeated slice preparation can therefore be handled through the machine’s controlled cutting process.
Specifications
	Model
	ZXG-300

	Cutting shaft speed
	200 - 1500r/min

	X cutting travel
	automatic 300mm

	Y cutting travel
	automatic 300mm

	X/Y speed
	0 - 100mm (stepless speed control)

	R axis speed
	1 - 100r/min

	Control system
	7-inch color touchscreen, PLC control system

	Cutting modes
	Automatic (single cutting, programmed slicing, continuous slicing and R-axis cutting)

	Feed method
	automatic 

	Effective feed travel
	300*300mm, R axis 360°

	Progress tracking
	LCD digital display (real-time)

	Cutting wire dimensions
	0.35 (0.2/0.25/0.35/0.5/1mm, etc.)

	Cutting speed
	0 - 5mm/min (stepless speed control)

	Cooling system
	automatic 30L

	Motor power
	3.0KW

	Power supply
	220V

	Dimensions
	900*720*1600mm (L * W * H)

	Net weight
	800KG

	Weight
	830KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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