[image: ]
Shanghai Microcre Optics-Mech Tech Co., Ltd.
SHANGHAI MICROCRE OPTICS-MECH TECH CO.,LTD  ·  www.cnnoet.com
Cold-mounting resin kit
Technical datasheet · Document MC-DS-64-EN · 2026-11-14
[image: ]
Product overview
The resin powder and hardener are mixed and poured into a mould for curing. The stated powder-to-liquid ratio is 5:4, with a stated curing time of 10–15 minutes.
Specifications
	Mounting powderCapacity 1kg
	

	Curing agentCapacity 1000ml
	


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
image2.jpg




image1.jpg
CCCCCCCCCCCCCCCCCCC








