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Product overview
The MP-2A uses waterproof abrasive papers and polishing materials for coarse grinding, fine grinding and polishing. Fixed-speed pairs of 500/1000 or 600/1200 rpm can be set at the factory to customer requirements; variable speed is adjustable from 100 to 1500 rpm. Two operators can work simultaneously, and a wash basin assists specimen cleaning. Suitable materials include metals and alloys, ceramics, rocks and electronic components.
Specifications
	Model
	MP-2A

	Machine body configuration
	Stainless steel cabinet, two discs and cleaning sink

	Control method
	Two discs with independent controls

	Rotation direction
	Forward and reverse rotation

	Grinding disc speed
	Stepless speed control (50-1500r/min) + preset speeds (400, 700, 900, 1400r/min)

	Main unit power
	550W*2

	Speed control
	Servo control

	Grinding disc diameter
	φ230mm (optional φ200)

	Water spray
	Adjustable orientation

	Power supply
	220V

	Dimensions
	1100*560*1050mm (L * W * H)

	Weight
	60KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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