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Product overview
The MP-3A uses waterproof metallographic abrasive papers of different grit sizes and polishing materials to prepare metal, alloy and petrographic specimens. Fixed-speed pairs of 500/1000 or 600/1200 rpm can be set at the factory to customer requirements. Variable operation provides an adjustable range of 100 to 1500 rpm, allowing the user to select a speed for either grinding or polishing.
Specifications
	Model
	MP-3A

	Machine body configuration
	Stainless steel cabinet, three discs and cleaning sink

	Control method
	Three discs with independent controls

	Rotation direction
	Forward and reverse rotation

	Grinding disc speed
	Stepless speed control (50-1500r/min) + preset speeds (400, 700, 900, 1400r/min)

	Main unit power
	550W*3

	Speed control
	Servo control

	Grinding disc diameter
	φ230mm (optional φ200)

	Water spray
	Adjustable orientation

	Power supply
	220V

	Dimensions
	1500*560*1050mm (L * W * H)

	Weight
	90KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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