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Product overview
The Q-2 sections specimens using a thin abrasive wheel rotating at high speed. It is intended for routine cutting of metal materials in metallographic laboratories and can also cut non-metallic materials such as plastics and rubber tubing. A cooling device can be fitted to carry away cutting heat and help limit heat-related changes to the specimen during preparation.
Specifications
	Model
	Q-2

	Maximum cutting diameter
	Φ35mm

	Cut-off wheel dimensions
	Φ250*1.5*Φ32mm

	Cutting modes
	manual 

	Spindle speed
	2800r/min

	Motor power
	1.1KW

	Machine configuration
	Benchtop

	Power supply
	380V

	Weight
	60KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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