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Product overview
An 8-inch colour touchscreen and PLC control operate the ZMP-3000Z grinding and polishing cycle. After grinding is completed, the machine automatically switches to polishing. Timed cooling-water spraying and automatic addition of grinding and polishing fluid are coordinated throughout the process. The arrangement reduces the manual intervention required to move between the grinding and polishing stages of specimen preparation.
Specifications
	Model
	ZMP-3000Z

	Machine body configuration
	Benchtop, three discs (automatic head locking)

	Clamping capacity
	8 specimens (30mm*6+40mm*2; custom specimen sizes available)

	Grinding and polishing configuration
	One-button operation with automatic changeover between grinding and polishing

	Pressure application
	Central loading / pneumatic individual loading

	Control method
	Color touchscreen, PLC control

	Operating system
	One-button operation (no operator intervention during the cycle)

	Grinding/polishing speed
	Stepless speed control (50-1500 rpm)

	Grinding head speed
	20-200 rpm (automatic speed control)

	Grinding and polishing method
	intelligent  / automatic  / manual 

	Preparation settings
	Stores up to 100 grinding and polishing programs

	Pressure loading
	Automatic loading and programmed changeover

	Abrasive dosing
	Programmed automatic dosing

	Dosing time
	Programmable; minimum spray duration 0.1S

	Dosing interval
	Programmable; minimum dosing interval 0.1S

	Cooling method
	water cooled

	Grinding/polishing changeover
	Automatic changeover without manually moving the head

	Preparation time
	0-9999 s *3

	Main unit power
	1000W*3

	Specimen preparation diameter
	30mm*6+40mm*2 (special sizes optional)

	Grinding disc diameter
	Choice of Φ230mm or Φ200mm

	Power supply
	220V/50HZ

	Dimensions
	1200*800*700mm (L * W * H)

	Net weight
	150KG

	Gross weight
	170KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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