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Product overview
The ZQ-150F is designed for precision sectioning of irregularly shaped workpieces. It supports metallographic sampling, slotting, thin flat slicing and segment cutting, with applications including automotive components, castings and specimens with particular positioning requirements. Available cutting approaches include vertical, layered, coordinated and manual operation, allowing the cutting approach to be selected to suit the workpiece and sampling task.
Specifications
	Model
	ZQ-150F

	Cutting chamber
	Right-side cutting chamber

	Main functions
	Cutting, precision slicing and fixed-depth grooving

	Spindle speed
	100 - 3000r/min (stepless speed control)

	X table movement
	manual 50mm (optional automatic )

	X axis speed
	0 - 100mm (stepless speed control)

	Z travel
	150mm

	Z axis speed
	0 - 200mm

	Y travel
	automatic /manual 250mm

	Y table speed
	0 - 200m (stepless speed control)

	Control system
	8-inch color touchscreen, PLC control system

	Maximum cutting diameter
	Φ110mm

	Disc workpiece cutting size
	200*80mm (outside diameter*height)

	Cutting modes
	Vertical, layered, horizontal and coordinated cutting (optional)

	Feed method
	Adjustable advance/retract ratio

	Effective feed travel
	110 + 200mm

	Progress tracking
	LCD digital display (real-time)

	Cutting table dimensions
	200*300mm

	Maximum wheel dimensions
	Φ350*2.5*Φ32mm

	Cutting speed
	1 - 200mm/min

	Clamping table
	Split, two-level movable table

	Speed adjustment during operation
	adjustable (1 - 100mm/min)

	Reset method
	Automatic reset with progress tracking

	Cooling system
	Automatic water cooling, 4 channels

	Tank capacity
	60L

	Motor power
	4KW

	Machine configuration
	Integrated floor-standing unit

	Power supply
	380V

	Dimensions
	900*850*1400mm (L*W*H)

	Net weight
	330KG

	Gross weight
	380KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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