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Product overview
The ZQ-30D is designed for precision sampling of small components. It combines a floor-standing, high-speed cutting arrangement with a colour touchscreen and PLC control. Compatible specimen materials include metals, ceramics, glass, rocks, crystals and electronic components. Its role is to section these small workpieces for subsequent examination and material analysis, using the control system to operate the cutting process.
Specifications
	Model
	ZQ-30D

	Main functions
	Precision cutting and positioned cutting

	Spindle speed
	200 - 3000r/min (stepless speed control)

	X table movement
	manual 50mm

	Z travel
	/

	Y travel
	100mm (automatic )

	Control system
	color touchscreen, PLCcontrol system

	Maximum cutting diameter
	Φ30mm

	Cutting modes
	Horizontal cutting

	Feed method
	Adjustable advance/retract ratio

	Effective travel
	70mm

	Progress tracking
	LCD digital display (real-time)

	Cutting table dimensions
	135 * 200mm

	Maximum wheel dimensions
	Φ180 * 1.2 * Φ25.4mm

	Cutting speed
	1 - 200mm/min

	Speed adjustment during operation
	adjustable / automatic reset

	Cooling system
	Automatic recirculating water cooling

	Tank capacity
	40L

	Motor power
	750W

	Power supply
	220V

	Dimensions
	600 * 600 * 500mm (L * W * H)

	Net weight
	40KG

	Gross weight
	60KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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