[image: ]
Shanghai Microcre Optics-Mech Tech Co., Ltd.
SHANGHAI MICROCRE OPTICS-MECH TECH CO.,LTD  ·  www.cnnoet.com
ZQ-600Z Large automatic metallographic cutting machine
Technical datasheet · Document MC-DS-ZQ-600Z-EN · 2026-11-14
[image: ]
Product overview
A colour touchscreen and PLC control coordinate movement along the X, Y and Z axes. The ZQ-600Z provides vertical, layered, horizontal, coordinated and manual cutting modes for sectioning, slicing and slotting. It is intended for large specimens made from conventional, very hard or high-toughness metals, as well as ceramics, crystals, rocks and workpieces combining different materials.
Specifications
	Model
	ZQ-600Z

	Cutting chamber
	Extra-large cutting chamber open on both sides for placement and cutting of extra-long workpieces

	Door opening
	Side sliding door

	Spindle speed
	100 - 3000r/min (stepless speed control)

	X table movement
	automatic 50mm

	Y travel
	automatic 380mm

	Z travel
	automatic 250mm

	Control system
	8-inch color touchscreen, PLC control system

	Maximum cutting diameter
	Φ170mm

	Disc workpiece cutting size
	Φ500*160mm

	Cutting modes
	Vertical, layered, horizontal and coordinated cutting

	Feed method
	Adjustable advance/retract ratio

	Effective feed travel
	200 + 350mm

	Progress tracking
	LCD digital display (real-time)

	Cutting table dimensions
	880*450mm (stainless steel table)

	Maximum wheel dimensions
	Φ430*2.9*Φ32mm

	Clamping table
	Split, two-level movable table

	Cutting speed
	1 - 200mm/min (speed adjustment during operation/automatic reset)

	Cooling system
	Automatic water cooling, 6 channels

	Tank capacity
	100L

	Motor power
	7.5KW (Siemens motor)

	Power supply
	380V

	Dimensions
	1500*1500*1800mm (L * W * H)

	Net weight
	1200KG

	Gross weight
	1300KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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