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Product overview
The ZXG-100 is intended for sectioning special ceramics, crystals, electronic ceramic components, gemstones, rocks and glass. Its touchscreen PLC system controls the cutting process and supports preparation of square specimen bars as well as automatic successive cutting of thin slices. Both specimen formats are supported within the machine’s controlled cutting sequence for brittle-material sampling.
Specifications
	Model
	ZXG-100

	Cutting shaft speed
	200 - 1000r/min

	X cutting travel
	automatic 100mm

	Y cutting travel
	automatic 100mm

	X/Y speed
	0 - 100mm (stepless speed control)

	R axis speed
	Options

	Control system
	7-inch color touchscreen, PLC control system

	Cutting modes
	Automatic (single cutting and continuous slicing)

	Feed method
	automatic 

	Effective feed travel
	80*80mm

	Progress tracking
	LCD digital display (real-time)

	Cutting wire dimensions
	0.35 (0.2/0.25/0.35/0.5/1mm, etc.)

	Cutting speed
	0 - 5mm/min (stepless speed control)

	Cooling system
	automatic 20L

	Motor power
	1.0KW

	Power supply
	220V

	Dimensions
	900*700*850mm (L * W * H)

	Net weight
	200KG

	Weight
	220KG


Contact
Phone: 400-8127-833 / +86-21-58391850
Email: shanghai@yr17.net
Address: No.1478 Nanfeng Highway, Fengxian District, Shanghai, China
Website: www.cnnoet.com
Compiled from published product information. Final configuration follows the technical agreement; confirm options, fixtures and scope with an application engineer.
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